Hello lads.

I have bluetooth HC-06.

Connected via FTDI-USB adapter to PC.

I'm using Termite on Windows for serial communication.

Baud rate 9600.

When I send AT nothing happens.

But if I send AT+NAME I get a response from Bluetooth and I can also change its name.

All other commands don't work!

AT+BAUD, AT+PIN, AT+UART.. None!

Wiring (BT <-> FTDI-USB)

vcc - vcc (5V)

gnd - gnd

TX - RX

RX - TX

Do you know why?

Boot in AT mode.





